NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Kingdom of Saudi Arabia  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:** Saudi Standards, Metrology and Quality Organization (SASO)  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  Saudi Standards, Metrology and Quality Organization  P. O. BOX: 3437 Riyadh 11471  Tel: +966(11)2529999 Ext: (9070-9061)  Fax: +966(11)4520193  Email: [enquirypoint@saso.gov.sa](mailto:enquirypoint@saso.gov.sa) |
| **3.** | **Notified under** **Article 2.9.2 [X], 2.10.1 [****], 5.6.2 [****], 5.7.1 [****], other:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** ICS: 29.140 |
| **5.** | **Title, number of pages and language(s) of the notified document:** Energy efficiency, functionality and labelling requirements for lighting products - Part 2 (58 page(s), in English) |
| **6.** | **Description of content:** Specifies energy efficiency, functionality, marking information, energy efficiency labelling and hazardous substances for lamps and luminaires with a luminous flux above 60 lumens, incandescent lamps with a luminous flux above 12000 lumens, Halogen lamps with a luminous flux above 12000 lumens, Compact fluorescent lamps with integrated ballast (CLFi) with a luminous flux above 12000 Lumens, Compact fluorescent lamps without integrated ballast (CFLni), fluorescent Lamps (all types), high Intensity Discharge Lamps and LED Lamps (including 'retrofit LED lamps' with a luminous flux above 12000 Lumens). |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** To ensure energy efficiency, functionality, marking information, energy efficiency labelling and hazardous substances for lamps and luminaires with a luminous flux above 60 lumens, incandescent lamps with a luminous flux above 12000 lumens, Halogen lamps with a luminous flux above 12000 lumens, Compact fluorescent lamps with integrated ballast (CLFi) with a luminous flux above 12000 Lumens, Compact fluorescent lamps without integrated ballast (CFLni), fluorescent Lamps (all types), high Intensity Discharge Lamps and LED Lamps (including 'retrofit LED lamps' with a luminous flux above 12000 Lumens). |
| **8.** | **Relevant documents:** <http://www.saso.gov.sa/en/eservices/tbt/Pages/default.aspx> |
| **9.** | **Proposed date of adoption:** 6 months from the date of publication in the official gazette  **Proposed date of entry into force:** 6 months from the date of publication in the official gazette |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X] or address, telephone and fax numbers and email and website addresses, if available, of other body:**  Email: [enquirypoint@saso.gov.sa](mailto:enquirypoint@saso.gov.sa) Website: <http://www.saso.gov.sa/en/eservices/tbt/Pages/default.aspx>  <https://members.wto.org/crnattachments/2017/TBT/SAU/17_5303_00_e.pdf> |